
How to decode NDI signal from TAO 1pro via OBS

1. Please install the two plug-ins，you can download from this link:
https://www.dropbox.com/s/zxgx7jq5wtdiyvp/OBS%20NDI%20Plugin%20for%20Windows.zip?dl=0
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2. Please enable NDI function on TAO 1pro.
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3. Please add NDI source In OBS software.
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4. Please select RGBlink in the signal source.
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5.Now you can see the NDI source in OBS software.
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