How to decode NDI signal from TAO 1 pro via vMix
Please enable NDI function on TAO 1pro.
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Please add NDI source In vMix software.
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Please select RGBlinkndi in the NDI signal source
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4. Now you can see the NDI source in vMix software.

